Figure 2. Moving Range Chart

The mR (moving range) chart shows variation of the process over time by charting the differences between each contiguous data point in the X-chart. All data points under the upper control limit indicate the process was in control throughout the pilot period.